#!/bin/sh
#
# Board specific MAVLink startup script.
#------------------------------------------------------------------------------

# Start ADS-B receiver mavlink connection if console not present
if [ ! -e /dev/console ]
then
	mavlink start -d /dev/ttyS4 -b 57600 -m minimal
fi
