#!/bin/sh
#
# board specific defaults
#------------------------------------------------------------------------------

param set-default CBRK_IO_SAFETY 0

neopixel start
safety_button start
tone_alarm start
