#!nsh
#
# @name Generic Hexarotor x geometry
#
# @type Hexarotor x
#
# @output AUX1 feed-through of RC AUX1 channel
# @output AUX2 feed-through of RC AUX2 channel
# @output AUX3 feed-through of RC AUX3 channel
#
# @maintainer Anton Babushkin <anton@px4.io>
#

sh /etc/init.d/rc.mc_defaults

set MIXER hexa_x

# Need to set all 8 channels
set PWM_OUT 12345678
