#
# This file is autogenerated: PLEASE DO NOT EDIT IT.
#
# You can use "make menuconfig" to make any modifications to the installed .config file.
# You can then do "make savedefconfig" to generate a new defconfig file that includes your
# modifications.
#
# CONFIG_DEV_CONSOLE is not set
# CONFIG_MMCSD_HAVE_CARDDETECT is not set
# CONFIG_MMCSD_HAVE_WRITEPROTECT is not set
# CONFIG_MMCSD_MMCSUPPORT is not set
# CONFIG_SPI_CALLBACK is not set
# CONFIG_STM32_CCMEXCLUDE is not set
CONFIG_ARCH="arm"
CONFIG_ARCH_BOARD_CUSTOM=y
CONFIG_ARCH_BOARD_CUSTOM_DIR="../../../../boards/diatone/mamba-f405-mk2/nuttx-config"
CONFIG_ARCH_BOARD_CUSTOM_DIR_RELPATH=y
CONFIG_ARCH_BOARD_CUSTOM_NAME="px4"
CONFIG_ARCH_CHIP="stm32"
CONFIG_ARCH_CHIP_STM32=y
CONFIG_ARCH_CHIP_STM32F405RG=y
CONFIG_ARCH_INTERRUPTSTACK=768
CONFIG_ARMV7M_MEMCPY=y
CONFIG_ARMV7M_USEBASEPRI=y
CONFIG_BOARDCTL_RESET=y
CONFIG_BOARD_ASSERT_RESET_VALUE=0
CONFIG_BOARD_CRASHDUMP=y
CONFIG_BOARD_CUSTOM_LEDS=y
CONFIG_BOARD_LOOPSPERMSEC=16717
CONFIG_BOARD_RESET_ON_ASSERT=2
CONFIG_BUILTIN=y
CONFIG_CDCACM=y
CONFIG_CDCACM_IFLOWCONTROL=y
CONFIG_CDCACM_PRODUCTID=0x0001
CONFIG_CDCACM_PRODUCTSTR="DiatoneMambaF405 MK2"
CONFIG_CDCACM_RXBUFSIZE=600
CONFIG_CDCACM_TXBUFSIZE=2000
CONFIG_CDCACM_VENDORID=0x26ac
CONFIG_CDCACM_VENDORSTR="Diatone"
CONFIG_DEBUG_SYMBOLS=y
CONFIG_DEV_FIFO_SIZE=0
CONFIG_DEV_PIPE_SIZE=70
CONFIG_DISABLE_MQUEUE=y
CONFIG_DISABLE_POSIX_TIMERS=y
CONFIG_FAT_DMAMEMORY=y
CONFIG_FAT_LCNAMES=y
CONFIG_FAT_LFN=y
CONFIG_FAT_LFN_ALIAS_HASH=y
CONFIG_FDCLONE_STDIO=y
CONFIG_FS_BINFS=y
CONFIG_FS_CROMFS=y
CONFIG_FS_FAT=y
CONFIG_FS_FATTIME=y
CONFIG_FS_PROCFS=y
CONFIG_FS_PROCFS_REGISTER=y
CONFIG_FS_ROMFS=y
CONFIG_GRAN=y
CONFIG_GRAN_INTR=y
CONFIG_HAVE_CXX=y
CONFIG_HAVE_CXXINITIALIZE=y
CONFIG_I2C=y
CONFIG_I2C_RESET=y
CONFIG_IDLETHREAD_STACKSIZE=750
CONFIG_INIT_ENTRYPOINT="nsh_main"
CONFIG_INIT_STACKSIZE=3194
CONFIG_LIBC_MAX_EXITFUNS=1
CONFIG_LIBC_STRERROR=y
CONFIG_MEMSET_64BIT=y
CONFIG_MEMSET_OPTSPEED=y
CONFIG_MMCSD=y
CONFIG_MM_REGIONS=2
CONFIG_MTD=y
CONFIG_MTD_BYTE_WRITE=y
CONFIG_MTD_PARTITION=y
CONFIG_MTD_PROGMEM=y
CONFIG_MTD_W25=y
CONFIG_NSH_ARCHINIT=y
CONFIG_NSH_BUILTIN_APPS=y
CONFIG_NSH_CROMFSETC=y
CONFIG_NSH_DISABLE_BASENAME=y
CONFIG_NSH_DISABLE_DD=y
CONFIG_NSH_DISABLE_DIRNAME=y
CONFIG_NSH_DISABLE_HEXDUMP=y
CONFIG_NSH_DISABLE_LOSETUP=y
CONFIG_NSH_DISABLE_MKFIFO=y
CONFIG_NSH_DISABLE_MKRD=y
CONFIG_NSH_DISABLE_PUT=y
CONFIG_NSH_DISABLE_REBOOT=y
CONFIG_NSH_DISABLE_UNAME=y
CONFIG_NSH_DISABLE_WGET=y
CONFIG_NSH_DISABLE_XD=y
CONFIG_NSH_FATDEVNO=0
CONFIG_NSH_FILEIOSIZE=512
CONFIG_NSH_LINELEN=128
CONFIG_NSH_MAXARGUMENTS=15
CONFIG_NSH_MMCSDSPIPORTNO=2
CONFIG_NSH_NESTDEPTH=8
CONFIG_NSH_READLINE=y
CONFIG_NSH_ROMFSETC=y
CONFIG_NSH_ROMFSSECTSIZE=128
CONFIG_NSH_STRERROR=y
CONFIG_NSH_VARS=y
CONFIG_PIPES=y
CONFIG_PREALLOC_TIMERS=50
CONFIG_PRIORITY_INHERITANCE=y
CONFIG_PTHREAD_STACK_MIN=512
CONFIG_RAM_SIZE=196608
CONFIG_RAM_START=0x20000000
CONFIG_RAW_BINARY=y
CONFIG_RTC_DATETIME=y
CONFIG_SCHED_HPWORK=y
CONFIG_SCHED_HPWORKPRIORITY=249
CONFIG_SCHED_HPWORKSTACKSIZE=1280
CONFIG_SCHED_INSTRUMENTATION=y
CONFIG_SCHED_INSTRUMENTATION_EXTERNAL=y
CONFIG_SCHED_INSTRUMENTATION_SWITCH=y
CONFIG_SCHED_LPWORK=y
CONFIG_SCHED_LPWORKPRIORITY=50
CONFIG_SCHED_LPWORKSTACKSIZE=1632
CONFIG_SCHED_WAITPID=y
CONFIG_SEM_PREALLOCHOLDERS=32
CONFIG_SERIAL_TERMIOS=y
CONFIG_SIG_DEFAULT=y
CONFIG_SIG_SIGALRM_ACTION=y
CONFIG_SIG_SIGUSR1_ACTION=y
CONFIG_SIG_SIGUSR2_ACTION=y
CONFIG_SIG_SIGWORK=4
CONFIG_STACK_COLORATION=y
CONFIG_START_DAY=30
CONFIG_START_MONTH=11
CONFIG_STDIO_BUFFER_SIZE=32
CONFIG_STM32_ADC1=y
CONFIG_STM32_BBSRAM=y
CONFIG_STM32_BBSRAM_FILES=5
CONFIG_STM32_BKPSRAM=y
CONFIG_STM32_CCMDATARAM=y
CONFIG_STM32_DISABLE_IDLE_SLEEP_DURING_DEBUG=y
CONFIG_STM32_DMA1=y
CONFIG_STM32_DMA2=y
CONFIG_STM32_FLASH_PREFETCH=y
CONFIG_STM32_FLOWCONTROL_BROKEN=y
CONFIG_STM32_I2C2=y
CONFIG_STM32_I2CTIMEOMS=10
CONFIG_STM32_I2CTIMEOTICKS=10
CONFIG_STM32_JTAG_SW_ENABLE=y
CONFIG_STM32_OTGFS=y
CONFIG_STM32_PWR=y
CONFIG_STM32_RTC=y
CONFIG_STM32_RTC_HSECLOCK=y
CONFIG_STM32_RTC_MAGIC_REG=1
CONFIG_STM32_SAVE_CRASHDUMP=y
CONFIG_STM32_SDIO=y
CONFIG_STM32_SDIO_CARD=y
CONFIG_STM32_SERIALBRK_BSDCOMPAT=y
CONFIG_STM32_SERIAL_DISABLE_REORDERING=y
CONFIG_STM32_SPI1=y
CONFIG_STM32_SPI1_DMA=y
CONFIG_STM32_SPI1_DMA_BUFFER=512
CONFIG_STM32_SPI2=y
CONFIG_STM32_SPI2_DMA=y
CONFIG_STM32_SPI3=y
CONFIG_STM32_SPI_DMATHRESHOLD=8
CONFIG_STM32_TIM1=y
CONFIG_STM32_TIM5=y
CONFIG_STM32_UART4=y
CONFIG_STM32_USART1=y
CONFIG_STM32_USART6=y
CONFIG_STM32_USART_BREAKS=y
CONFIG_STM32_USART_SINGLEWIRE=y
CONFIG_STM32_WWDG=y
CONFIG_SYSTEM_CDCACM=y
CONFIG_SYSTEM_NSH=y
CONFIG_TASK_NAME_SIZE=24
CONFIG_UART4_BAUD=57600
CONFIG_UART4_RXBUFSIZE=600
CONFIG_UART4_TXBUFSIZE=600
CONFIG_USART1_RXBUFSIZE=300
CONFIG_USART1_RXDMA=y
CONFIG_USART1_TXBUFSIZE=300
CONFIG_USART6_BAUD=57600
CONFIG_USART6_RXBUFSIZE=300
CONFIG_USART6_RXDMA=y
CONFIG_USART6_TXBUFSIZE=300
CONFIG_USBDEV=y
CONFIG_USBDEV_BUSPOWERED=y
CONFIG_USBDEV_MAXPOWER=500
CONFIG_USEC_PER_TICK=1000
